For 1990-2009 cars

## Air Conditioning Clutch Coil Removal SP10 Compressor

1. Remove the clutch and drive assembly. Refer to Compressor Clutch Plate and Hub Assembly Removal .
2. Remove the pulley and bearing assembly. Refer to Clutch Rotor and Bearing Removal .
3. Remove the coil retainer using the snap ring pliers (1).
4. Remove the coil and housing assembly.

## Air Conditioning Clutch Coil Removal V5 Compressor

#### Special Tools

• | J 8433-1 Puller Crossbar

• | J 8433-3 Forcing Screw

• | J 33023-A Puller Pilot

• | J 33025 Clutch Coil Puller Legs

### Disassembly Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Recover the refrigerant. Refer to Refrigerant Recovery and Recharging.
3. Remove the compressor. Refer to Air Conditioning Compressor Replacement.
4. Remove the clutch plate and hub assembly. Refer to Compressor Clutch Plate and Hub Assembly Removal.
5. Remove the clutch rotor and bearing. Refer to Clutch Rotor and Bearing Removal.
6. Mark the clutch coil terminal location on the compressor housing.
7. Install the J 33023-A (1) on the compressor housing. Also install the J 8433-1 (3) with the J 33025 (4).
8. Tighten the J 8433-3 (2) against the J 33023-A (1) to remove the clutch coil.