For 1990-2009 cars

## Compressor Clutch Plate and Hub Assembly Removal V5 Compressor

#### Tools Required

• | J 33013-B Hub and Drive Plate Remover/Installer

• | J 33027-A Clutch Hub Holding Tool

• | J 42428 Compressor Holding Fixture

### Disassembly Procedure

1. Remove the compressor. Refer to Air Conditioning Compressor Replacement .
2. Install the J 42428 to the compressor and hold the compressor holding fixture using a bench vise.
3. Use the J 33027-A to keep the clutch drive plate and the hub assembly from turning. Remove the shaft nut.
4. Thread the J 33013-B (1) into the hub. Hold the body of the remover with a wrench and turn the center screw into the remover body to remove the clutch drive plate and hub assembly.
5. Remove the clutch hub key. Retain the key for assembly (3).

## Compressor Clutch Plate and Hub Assembly Removal SP10 Compressor

#### Tools Required

DW-610-010 Clutch Hub Holding Tool

1. Remove the compressor. Refer to Air Conditioning Compressor Replacement .
2. Use the DW-610-010 clutch hub holding tool (1) to keep the clutch drive assembly from turning.
3. Remove the shaft bolt.
4. Pull the clutch drive assembly up by hand.