For 1990-2009 cars

## Rear Compartment Lid Lock Cylinder Replacement Hatchback

### Removal Procedure

1. Remove the hatchback door lower garnish molding, if equipped.
2. Disconnect the lock rod.
3. Remove the nuts and the lock cylinder.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the lock cylinder with the nuts.

Tighten
Tighten the luggage compartment lock cylinder nuts to 3 N·m (27 lb in).

2. Connect the lock rod.
3. Install the hatchback door lower garnish molding, if equipped.