For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Disconnect the throttle position (TP) sensor connector.
3. Remove the TP sensor retaining bolts and the TP sensor.

### Installation Procedure

1. With the throttle valve closed, position the TP sensor on the throttle shaft. Align the TP sensor with the bolt holes.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the TP sensor retaining bolts.

Tighten
Tighten the throttle position sensor retaining bolts to 2 N·m (18 lb in).

3. Connect the TP sensor connector.
4. Connect the negative battery cable.