For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the cigar lighter from the cigar lighter housing.
3. Remove the floor console. Refer to Front Floor Console Replacement.
4. Remove the cigar lighter housing from the instrument panel.
5. Disconnect the cigar lighter electrical connector.

### Installation Procedure

1. Connect the cigar lighter electrical connector.
2. Install the cigar lighter housing in the instrument panel.
3. Install the floor console. Refer to Front Floor Console Replacement.
4. Install the cigar lighter in the cigar lighter housing.
5. Connect the negative battery cable.