For 1990-2009 cars

### Removal Procedure

Warning: Refer to Relieving Fuel Pressure Warning in the Preface section.

1. Relieve the fuel system pressure. Refer to Fuel Pressure Relief.
2. Remove the fuel pump assembly. Refer to Fuel Pump Replacement.
3. Disconnect the insulator connector.

Note: The wedge may be disconnected with severe force but can be reconnected.

4. Push the terminal wedge (1) in the insulator connector.
5. Remove the fuel level sensor (1) from the sender housing (2).
6. Remove the sender housing.
7. Remove the fuel sender assembly (3).

### Installation Procedure

1. Install the wires (1) into the sender assembly (2).

Note: Ensure the sender assembly and the fuel level sensor are installed properly. If not the fuel gauge and fuel level warning indicator will not function properly.

2. Install the sender assembly onto the fuel pump assembly (1).
3. Install the fuel level sensor onto the sender housing.
4. Connect the wire into the insulator connector.
5. Connect the insulator connector
6. Install the fuel pump assembly into the fuel tank. Refer to Fuel Pump Replacement.