For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
A/C Compressor Mounting Bolts | 27 N·m | 20 lb ft
A/C Compressor Mounting Bracket Bolts | 50 N·m | 37 lb ft
Air Filter Housing Bolts | 12 N·m | 106 lb in
Alternator Adjusting Bolt | 20 N·m | 15 lb ft
Alternator Adjusting Bracket Retaining Bolt | 20 N·m | 15 lb ft
Auxiliary Catalytic Converter-to-Exhaust Manifold Nuts and Bracket Bolts | 40 N·m | 30 lb ft
Camshaft Cap Bolts | 16 N·m | 12 lb ft
Camshaft Gear Bolt | 67.5 N·m | 49 lb ft
Camshaft Pressure Plate Bolts | 10 N·m | 89 lb in
Connecting Rod Bearing Cap Bolts | 25 N·m+30°+15° | 18 lb ft+30°+15°
Coolant Pump Retaining Bolts | 10 N·m | 89 lb in
Coolant Temperature Sensor | 20 N·m | 15 lb ft
Crankshaft Bearing Cap Bolts | 50 N·m+45°+15° | 37 lb ft+45°+15°
Crankshaft Position Sensor Retaining Bolt | 10 N·m | 89 lb in
Crankshaft Pulley Bolt | 95 N·m+30°+15° | 70 lb ft+30°+15°
Cylinder Head Bolts - Camshaft Support Housing and Cylinder Head Mounting Bolts | 25 N·m+60°+60°+60°+15° | 18 lb ft+60°+60°+60°+10°
Electronic Ignition System Ignition Coil Mounting Bolts | 10 N·m | 89 lb in
Electronic Ignition System Ignition Coil Mounting Plate Bolts | 10 N·m | 89 lb in
Engine Mount Bracket Retaining Bolt | 65 N·m | 48 lb ft
Engine Mount Bracket-to-Engine Mount Retaining Bolts | 60 N·m | 44 lb ft
Engine Mount Retaining Nuts | 40 N·m | 30 lb ft
Exhaust Flexible Pipe Bracket Bolts | 40 N·m | 30 lb ft
Exhaust Gas Recirculation Valve Adapter Bolts | 25 N·m | 18 lb ft
Exhaust Manifold Heat Shield Bolts | 15 N·m | 11 lb ft
Exhaust Manifold Nuts | 25 N·m | 18 lb ft
Flexible Plate Bolts | 60 N·m | 44 lb ft
Flexible Plate Inspection Cover Bolts | 10 N·m | 89 lb in
Flywheel Bolts | 35 N·m+30°+15° | 26 lb ft+30°+15°
Flywheel Inspection Cover Bolts | 12 N·m | 106 lb in
Front Muffler-to-Main Catalytic Converter Nuts | 30 N·m | 22 lb ft
Fuel Rail Retaining Bolts | 25 N·m | 18 lb ft
Intake Manifold Retaining Nuts | 25 N·m | 18 lb ft
Intake Manifold Support Bracket Lower Bolt-to-Engine Block | 40 N·m | 30 lb ft
Intake Manifold Support Bracket Upper Bolts | 25 N·m | 18 lb ft
Lower Timing Belt Cover Bolts | 10 N·m | 89 lb in
Oil Pan Drain Plug | 55 N·m | 40 lb ft
Oil Pan Retaining Bolts | 10 N·m | 89 lb in
Oil Pressure Switch | 40 N·m | 30 lb ft
Oil Pump Retaining Bolts | 10 N·m | 89 lb in
Oil Pump/Pickup Tube and Support Bracket Bolts | 10 N·m | 89 lb in
Oil Pump Safety Relief Valve Bolt | 36 N·m | 22 lb ft
Oil Pump Rear Cover Bolts | 6 N·m | 53 lb in
Power Steering Pump Mounting Bolts | 25 N·m | 18 lb ft
Power Steering Pump Pulley Bolts | 25 N·m | 18 lb ft
Rear Timing Belt Cover Bolts | 10 N·m | 89 lb in
Spark Plug Cover Bolts | 3 N·m | 27 lb in
Spark Plugs | 25 N·m | 18 lb ft
Thermostat Housing Mounting Bolts | 20 N·m | 15 lb ft
Throttle Cable Bracket Bolts | 8 N·m | 71 lb in
Timing Belt Automatic Tensioner Bolt | 25 N·m | 18 lb ft
Timing Belt Idler Pulley Bolt | 40 N·m | 30 lb in
Transaxle Bell Housing Bolts | 75 N·m | 55 lb ft
Transaxle Brace Bolts | 40 N·m | 30 lb ft
Transaxle Torque Converter Bolts | 65 N·m | 48 lb ft
Upper Timing Belt Cover Bolts | 10 N·m | 89 lb in
Valve Cover Bolts | 10 N·m | 89 lb in