For 1990-2009 cars

## Radio Antenna Module Replacement Notchback

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement .
3. Disconnect the negative battery cable.
4. Remove the screws and the glass antenna module.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the glass antenna module with the screws.

Tighten
Tighten the roof antenna retaining screws to 2.5-3.5 N·m (22-31 lb in).

2. Connect the electrical connectors.
3. Install the rear quarter upper trim panel. Refer to Quarter Upper Trim Panel Replacement .
4. Connect the negative battery cable.

## Radio Antenna Module Replacement Hatchback

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the interior courtesy lamp. Refer to Interior Courtesy Lamp Replacement .
3. Remove the screw from the vehicle inside.
4. Remove the roof antenna.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the roof antenna with the screw.

Tighten
Tighten the roof antenna retaining screws to 3 N·m (27 lb in).

2. Install the interior courtesy lamp. Refer to Interior Courtesy Lamp Replacement .
3. Connect the negative battery cable.