For 1990-2009 cars

Icon | Icon Definition
--- | ---
| Caution: When performing service on or near the SIR components or the SIR wiring, the SIR system must be disabled. Refer to SIR Disabling and Enabling . Failure to observe the correct procedure could cause deployment of the SIR components, personal injury, or unnecessary SIR system repairs.
| Important:

• | In order to prevent accidental deployment, the shorting bars close in order to short the connectors when the connectors are separated.

• | Twisted-pair wires provide an effective shield that helps protect sensitive electronic components from electrical interference. If the wires were covered with shielding, install new shielding.

| In order to prevent electrical interference from degrading the performance of the connected components, you must maintain the proper specification when making any repairs to the twisted-pair wires shown :

- | The wires must be twisted a minimum of 9 turns per 31 cm (12 in) as measured anywhere along the length of the wires

- | The outside diameter of the twisted wires must not exceed 6.0 mm (0.25 in)