For 1990-2009 cars

Table 1: | Camshaft Position (CMP) Sensor
Table 2: | Crankshaft Position (CKP) Sensor
Table 3: | Engine Coolant Temperature (ECT) Sensor
Table 4: | Evaporative Emission (EVAP) Canister Purge Solenoid Valve
Table 5: | Evaporative Temperature Sensor
Table 6: | Exhaust Gas Recirculation (EGR) Valve
Table 7: | Fuel Injector 1
Table 8: | Fuel Injector 2
Table 9: | Fuel Injector 3
Table 10: | Fuel Injector 4
Table 11: | Fuel Pump/Sender
Table 12: | Heated Oxygen Sensor (HO2S) 1
Table 13: | Heated Oxygen Sensor (HO2S) 2
Table 14: | Ignition Coil Module
Table 15: | Intake Air Temperature (IAT) Sensor
Table 16: | Knock Sensor (KS)
Table 17: | Manifold Absolute Pressure (MAP) Sensor
Table 18: | Octane Selection Switch
Table 19: | Oxygen (O2) Sensor
Table 20: | Throttle Body - Main Throttle Idle Actuator (MTIA)

#### Camshaft Position (CMP) Sensor

Connector Part Information |

• | AMP 85205-1

• | 3-Way F JR Power Timer 3P Housing Assembly (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU/BK | 1749 | Low Reference
2 | L-GN/WH | 1748 | Camshaft Position (CMP) Sensor Signal
3 | BN | 1733 | Ignition 1 Voltage

#### Crankshaft Position (CKP) Sensor

Connector Part Information |

• | AMP 85205-1

• | 3-Way F JR Power Timer 3P Housing Assembly (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-BU/WH | 1869 | Crankshaft Position (CKP) Sensor Signal
2 | YE/BK | 1868 | Low Reference
3 | BK/WH | 51 | Ground

#### Engine Coolant Temperature (ECT) Sensor

Connector Part Information |

• | PED 12040753

• | 2-Way F Metri-Pack 150 Series Sealed, Pull To Seat (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | L-BN | 410 | Engine Coolant Temperature (ECT) Sensor Signal
B | D-GN | 808 | Low Reference

#### Evaporative Emission (EVAP) Canister Purge Solenoid Valve

Connector Part Information |

• | AMP 85202-1

• | 2-Way F JR Power Timer 2P Housing Assembly (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BK | 452 | Evaporative Emission (EVAP) Canister Purge Valve Solenoid Control
2 | OG/BK | 1733 | Ignition 1 Voltage

#### Evaporative Temperature Sensor

Connector Part Information |

• | KET MG 610392

• | 2-Way F Sealed Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | 732 | Evaporator Temperature Sensor Signal
2 | L-BU | 733 | Low Reference

#### Exhaust Gas Recirculation (EGR) Valve

Connector Part Information |

• | AMP 174262-2

• | 6-Way F Econoseal J-Mark II + 6P (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN/WH | 416 | 5-Volt Reference
2 | D-GN | 813 | Low Reference
3 | D-GN | 435 | Exhaust Gas Recirculation (EGR) Valve Control
4 | BN | 1733 | Ignition 1 Voltage
5 | -- | -- | Not Used
6 | D-BU | 436 | Exhaust Gas Recirculation (EGR) Valve Control

#### Fuel Injector 1

Connector Part Information |

• | AMP 368468-1

• | 2-Way F Injector Plug Assembly (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | 1733 | Ignition 1 Voltage
2 | BN/BK | 1747 | Fuel Injector 1 Control

#### Fuel Injector 2

Connector Part Information |

• | AMP 368468-1

• | 2-Way F Injector Plug Assembly (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | 1733 | Ignition 1 Voltage
2 | BN/BK | 1746 | Fuel Injector 2 Control

#### Fuel Injector 3

Connector Part Information |

• | AMP 368468-1

• | 2-Way F Injector Plug Assembly (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | 1733 | Ignition 1 Voltage
2 | YE/D-BU | 1745 | Fuel Injector 3 Control

#### Fuel Injector 4

Connector Part Information |

• | AMP 368468-1

• | 2-Way F Injector Plug Assembly (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | BN | 1733 | Ignition 1 Voltage
2 | L-GN/BK | 1744 | Fuel Injector 4 Control

#### Fuel Pump/Sender

Connector Part Information |

• | AMP 936039

• | 6-Way F Fuel Pump 6POS Conn'r Assembly (BN)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | GY | 1936 | Fuel Level Sensor Signal
2 | BK | 850 | Ground
3 | BN | 1723 | Fuel Pump Supply Voltage
4 | BN | 850 | Ground
5 | PU | 172 | Low Fuel Indicator Signal
6 | L-BU | 1937 | Low Reference

#### Heated Oxygen Sensor (HO2S) 1

Connector Part Information |

• | KUM PB 625-04027

• | 4-Way F NMWP 02F-B Assembly (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN/WH | 428 | Low Reference
2 | BN/WH | 50 | Heated Oxygen Sensor (HO2S) 1 Signal
3 | OG | 469 | Heated Oxygen Sensor (HO2S) 1 Heater Control
4 | BN | 1733 | Ignition 1 Voltage

#### Heated Oxygen Sensor (HO2S) 2

Connector Part Information |

• | AMP 174257-2

• | 4-Way M 070 Series Econoseal J MK-2 Plug Assembly 4P (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | PU | 1670 | Heated Oxygen Sensor (HO2S) 2 Low Reference
2 | PU | 1671 | Heated Oxygen Sensor (HO2S) 2 Signal
3 | L-BU | 733 | Heated Oxygen Sensor (HO2S) 2 Heater Control
4 | BN | 1733 | Ignition 1 Voltage

#### Ignition Coil Module

Connector Part Information |

• | PED 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | WH | 423 | Ignition Coil 2 and 3 Control
B | PK | 539 | Ignition 1 Voltage
C | OG | 406 | Ignition Coil 1 and 4 Control

#### Intake Air Temperature (IAT) Sensor

Connector Part Information |

• | AMP 85202-1

• | 2-Way F JR Power Timer 2P Housing Assembly (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | L-BU | 468 | Intake Air Temperature (IAT) Sensor Signal
2 | D-GN | 808 | Low Reference

#### Knock Sensor (KS)

Connector Part Information |

• | AMP 368215-1

• | 3-Way F JPT 3P Assembly for Knock Sensor (GY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | YE/BK | 496 | Knock Sensor (KS) Signal
2 | D-BU | 1876 | Low Reference
3 | BK | 51 | Ground

#### Manifold Absolute Pressure (MAP) Sensor

Connector Part Information |

• | PED 12059595

• | 3-Way F Metri-Pack 150 Series Sealed (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | OG/BK | 469 | Low Reference
B | GY/BK | 433 | Manifold Absolute Pressure (MAP) Sensor Signal
C | L-BU/WH | 432 | 5-Volt Reference

#### Octane Selection Switch

Connector Part Information |

• | KET MG 620395

• | 3-Way M Sealed Series (WH)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN | 890 | Octane Switch Signal
2 | BK | 51 | Ground
3 | BN | 1456 | Octane Switch Signal

#### Oxygen (O2) Sensor

Connector Part Information |

• | AMP 174352-2

• | 2-Way M Econoseal J Mark II + Connector Plug Housing (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | D-GN/WH | 428 | Oxygen (O2) Sensor Signal
2 | BK | 469 | Low Reference

#### Throttle Body - Main Throttle Idle Actuator (MTIA)

Connector Part Information |

• | AMP 174982-2

• | 8-Way M 070 Series Econoseal J-Mark II + 8P (BK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
1 | WH/BN | 425 | Idle Motor Speed Return
2 | WH/D-BU | 533 | 5-Volt Reference
3 | -- | -- | Not Used
4 | L-GN/WH | 534 | Idle Motor Position Signal
5 | D-BU | 426 | Idle Motor Speed Signal
6 | PU | 427 | Idle Switch Position Signal
7 | L-GN | 417 | Throttle Position (TP) Sensor Signal
8 | GN | 415 | Low Reference