For 1990-2009 cars

Checks | Actions
--- | ---
Check the steering gear-to-column joints for improper installation. | Tighten the coupling flange pinch bolts. Replace the coupling flange as needed.
Check for column misalignment. | Replace the alignment spacer.
Check the steering shaft bearing for wear or damage. | Replace the steering shaft bearing.
Check the spherical joint for lack of lubrication. | Lubricate the spherical joint.
Check the steering shaft for lack of lubrication. | Lubricate the steering shaft bearing.
Check the shaft lock snap ring for improper seating. | Adjust the shaft lock snap ring. Replace the shaft lock snap ring as needed.