For 1990-2009 cars

#### Tools Required

J 28467-B (DW-117) Universal Engine Support Fixture

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

Notice: Refer to Engine Mounting Notice in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the air cleaner housing bolts and the air filter housing assembly.

Notice: When raising or supporting the engine for any reason, do not use a jack under the oil pan, any sheet metal, or crankshaft balancer. Jacking against the oil pan may cause it to crack or break.

3. Support the engine assembly using the J 28467-B .
4. Remove the engine mount bracket retaining bolts (1).
5. Remove the engine mount attaching nuts (1).
6. Remove the engine mount.

### Installation Procedure

1. Install the engine mount.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the engine mount attaching nuts (1).

Tighten
Tighten the engine mount attaching nuts to 40 N·m (30 lb ft).

3. Install the engine mount bracket retaining bolts (1).

Tighten
Tighten the engine mount bracket retaining bolts to 60 N·m (44 lb ft).

4. Remove the J 28467-B .
5. Connect the negative battery cable.