For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the air cleaner assembly.
3. Disconnect the crankshaft position (CKP) sensor connector.
4. Remove the CKP sensor retaining bolt.
5. Remove the CKP sensor.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the CKP sensor with the retaining bolt.

Tighten
Tighten the CKP sensor retaining bolt to 6.5 N·m (58 lb in).

2. Connect the CKP sensor connector.
3. Install the air cleaner assembly.
4. Connect the negative battery cable.