For 1990-2009 cars

### Removal Procedure

Caution: Refer to Liftgate Assist Rod Caution in the Preface section.

1. Open and suitably support the hatchback door.
2. Unscrew and remove the gas support assembly from the hatchback door and the body.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the gas support assembly onto the hatchback door and the body and tighten to 8 N·m (71 lb in).
2. Close the hatchback door.