For 1990-2009 cars

#### Special Tools

EN-49073 Timing Chain Tensioner

### Removal Procedure

1. Install the timing chain after aligning both the mark (1) on the camshaft sprocket and on the timing chain.
2. Align both the timing mark (2) on the crankshaft sprocket and on the timing chain.
3. Push the timing chain tensioner lever and fix the lever by installing the tensioner pin EN-49073 (2).

Caution: Refer to Fastener Caution in the Preface section.

4. Assemble the timing chain guide (1).

Tighten
Tighten the timing chain guide retaining bolts to 10 N·m (7.4 lb in).

5. Assemble the timing chain lever (4).

Tighten
Tighten the timing chain lever retaining bolts to 10 N·m (7.4 lb in).

6. Assemble the timing chain tensioner (3).

Tighten
Tighten the timing chain tensioner retaining bolts to 12 N·m (8.8 lb in).

### Installation Procedure

Install the timing chain cover (1).

Tighten

• | Tighten the timing chain cover retaining bolts (M6 x 1.0) to 10.5 N·m (7.7 lb in).

• | Tighten the timing chain cover retaining bolts (M8 x 1.25) to 20 N·m (14.7 lb ft).