For 1990-2009 cars

### Inspection Procedure

1. Remove the brake drum. Refer to Brake Drum Replacement.

Warning: Refer to Brake Dust Warning in the Preface section.

2. Measure the lining thickness.

Specification
The minimum lining thickness is 0.5 mm (0.02 in).

Note: Replace the shoe and lining assembly in axle sets only.

3. If the lining thickness is less than the specification, or if a defect is found, replace the linings. Refer to Brake Shoe Replacement.
4. Install the brake drum. Refer to Brake Drum Replacement.