For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Drums

- Inside Diameter - New

200 mm

7.87 in

- Maximum Inside Diameter

201 mm

7.91 in

- Maximum Radial Runout - Not Installed

0.04 mm

0.002 in

Wheel Cylinder Diameter - Rear | 20.64 mm | 0.81 in
Brake Rotors

- Disc Type

Ventilated

- Discard Thickness for 236 mm (9.29 in) Diameter Rotor

18 mm

0.709 in

- Discard Thickness for 256 mm (10.08 in) Diameter Rotor

22 mm

0.866 in

- Maximum Assembled Lateral Runout - Installed

0.06 mm

0.002 in

- Maximum Groove Depth

0.40 mm

0.016 in

- Maximum Lateral Runout - Not Installed

0.03 mm

0.001 in

- Maximum Thickness Variation

0.10 mm

0.004 in

- New Rotor Thickness - 236 mm (9.29 in) Diameter Rotor

20 mm

0.787 in

- New Rotor Thickness - 256 mm (10.08 in) Diameter Rotor

24 mm

0.945 in

- Rotor Diameter - Larger Size with SACL500 Stamping

256 mm

10.08 in

- Rotor Diameter - Smaller Size with SACL485F Stamping

236 mm

9.29 in

Booster Ratio | 5:1
Booster Size | 241.3 mm | 9.5 in
Master Cylinder

- Bore Diameter

22.22 mm

0.87 in

- Minimum Bore Diameter

20.64 mm

0.81 in

Caliper

- Piston Minimum Diameter

54 mm

2.12 in