For 1990-2009 cars

## Front Floor Console Replacement Notchback

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the gearshift lever boot, if equipped.
3. Remove the screws from the floor console.
4. Remove the floor console cover.
5. Remove the parking brake cover.
6. Disconnect the electrical connector.
7. Remove the floor console.

### Installation Procedure

1. Connect the electrical connector.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the floor console with the screws and tighten to 4 N·m (35 lb in).
3. Install the parking brake cover.
4. Install the floor console cover.
5. Install the gearshift lever boot, if equipped.
6. Connect the negative battery cable.