For 1990-2009 cars

### Removal Procedure

1. Siphon the power steering fluid from the reservoir.
2. Disconnect the suction hose from the power steering pump.
3. Disconnect the suction hose from the reservoir.
4. Remove the suction pipe retaining clamp nuts (1, 2) under the radiator.
5. Remove the suction hose from the vehicle.

### Installation Procedure

1. Connect the suction hose to the reservoir.
2. Connect the suction hose to the power steering pump.

Caution: Refer to Fastener Caution in the Preface section.

3. Install the suction pipe retaining clamp nuts (1, 2). Tighten the nuts to 8 N·m (70 lb in).
4. Fill the power steering fluid reservoir and bleed the power steering system. Refer to Power Steering System Bleeding.