For 1990-2009 cars

### Removal Procedure

1. Drain the engine coolant. Refer to Cooling System Draining and Filling.
2. Release the fuel pressure. Refer to Fuel Pressure Relief.
3. Remove the timing belt. Refer to Timing Belt Replacement.
4. Remove the timing belt tensioner. Refer to Timing Belt Replacement.
5. Remove the camshaft. Refer to Camshaft Gear Replacement.
6. Remove the timing belt rear cover (1).
7. Remove the intake manifold. Refer to Intake Manifold Replacement.
8. Remove the exhaust manifold. Refer to Catalytic Converter Replacement.
9. Remove the coolant distributor (1).
10. Remove the cylinder head bolts (1).
11. Remove the cylinder head (2) with the gasket.

### Installation Procedure

1. Install the cylinder head (2) with the new gasket.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the cylinder head bolts (1) and tighten to 25 N·m +90° +90° +90° +45° (18.4 lb ft +90° +90° +90° +45° ).
3. Install the coolant distributor (1).
4. Install the exhaust manifold. Refer to Catalytic Converter Replacement.
5. Install the intake manifold. Refer to Intake Manifold Replacement.
6. Install the timing belt rear cover (1) and tighten to 6 N·m (53.1 lb in).
7. Install the camshaft. Refer to Camshaft Replacement.
8. Adjust the belt timing. Refer to Timing Belt Replacement.