For 1990-2009 cars

### Removal Procedure

Notice: Refer to Vehicle Lifting and Jacking Notice in the Preface section.

1. Raise and suitably support the vehicle.
2. Remove the front wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Remove the nuts, the bolts, and the engine under cover.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the engine under cover with the bolts and nuts.

Tighten
Tighten the engine under cover nuts and bolts to 3.5 N·m (31 lb in).

2. Install the front wheel. Refer to Tire and Wheel Removal and Installation in Tires and Wheels.
3. Lower the vehicle.