For 1990-2009 cars

### Removal Procedure

1. Remove the rotor. Refer to Brake Rotor Replacement.
2. Remove the screws for the splash shield from the steering knuckle.
3. Remove the splash shield.

### Installation Procedure

1. Install the splash shield.

Caution: Refer to Fastener Caution in the Preface section.

2. Secure the splash shield to the steering knuckle with the screws and tighten to 4 N·m (35 lb in).
3. Install the rotor. Refer to Brake Rotor Replacement.