For 1990-2009 cars

### Removal Procedure

1. Drain the engine oil. Refer to Engine Oil and Oil Filter Replacement.
2. Remove the front exhaust pipe. Refer to Front Pipe Replacement.
3. Remove the transmission rear mounting bracket (2), for automatic transmission only.
4. Remove the oil pan-to-transmission bolts (1).
5. Remove the oil pan bolts (1).
6. Remove the oil pan baffle (2).
7. Remove the oil suction filter (3).

### Installation Procedure

1. Install the oil suction filter (3) to the oil pan.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the oil pan baffle (2).

Tighten
Tighten the oil pan baffle bolts (1) to 10 N·m (7.3 lb ft).

3. Clean the oil pan sealing surface.
4. Apply the oil pan sealant LOCTITE 5900 on the sealing surface.
5. Install the oil pan bolts (1).

Tighten
Tighten the oil pan bolts (1) to 14 N·m (10.3 lb ft).

6. Install the oil pan-to-transmission bolts (1).

Tighten
Tighten the oil pan-to-transmission bolts (1) to 40 N·m (29.5 lb ft).

7. Install the transmission rear mounting bracket (2), for automatic transmission only.

Tighten
Tighten the transmission rear mounting bracket bolts and nut to 80 N·m (59 lb ft).