For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

Note: Information must be retrieved from the instrument cluster before removing. Refer to Control Module References.

1. Disconnect the negative battery cable.
2. Remove the instrument cluster trim panel.
3. Remove the instrument cluster rear trim panel.
4. Remove the screws and the instrument cluster.
5. Disconnect the electrical connectors.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Connect the electrical connectors.
2. Install the instrument cluster with the screws and tighten to 4 N·m (35 lb in).
3. Install the instrument cluster rear trim panel.
4. Install the instrument cluster trim panel.
5. Connect the negative battery cable.
6. Program the instrument cluster. Refer to Control Module References.