For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel (I/P) center trim panel.
2. Remove the I/P accessory bezel.
3. Remove the I/P stow tray.
4. Remove the front radio speaker and grille.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the front radio speaker with the screws and tighten to 2 N·m (18 lb in).
2. Install the front radio speaker grille.
3. Install the I/P stow tray with the screws and tighten to 2 N·m (18 lb in).
4. Install the I/P accessory bezel with the screws and tighten to 2 N·m (18 lb in).