For 1990-2009 cars

### Removal Procedure

1. Remove the center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement .
2. Remove the screws holding the shift indicator to the center console trim bezel and disconnect the electrical connector.
3. Remove the shift indicator from the center trim bezel.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Align the shift indicator with the center trim bezel and fasten with the screws.

Tighten
Tighten the screws to 2 N·m (18 lb in).

2. Connect the electrical connection to the center trim bezel.
3. Install the center trim bezel. Refer to Instrument Panel Accessory Bezel Replacement .