For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable. Battery Negative Cable Disconnection and Connection.
2. Remove the front bumper fascia. Refer to Front Bumper Fascia Replacement.
3. Remove the screws that secure the fog lamp assembly.
4. Disconnect the fog lamp assembly electrical connector.
5. Remove the fog lamp assembly.
6. Remove the bulb from the fog lamp assembly, if necessary.

### Installation Procedure

1. Install the bulb to the fog lamp assembly, if removed.
2. Install the fog lamp assembly with the screws.
3. Connect the electrical connector.
4. Install the front bumper fascia. Refer to Front Bumper Fascia Replacement.
5. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection.