For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Blower Motor Resistor Screws | 6 N·m | 53 lb in
Blower Motor Screws | 6 N·m | 53 lb in
Clutch Plate and Hub Assembly Retaining Nut | 13.5 N·m | 10 lb ft
Compressor Hose Bracket-to-Vehicle Bolt | 9 N·m | 80 lb in
Compressor Hose-to-Compressor Nut | 16 N·m | 12 lb ft
Compressor Hose-to-Condenser Bolt | 16 N·m | 12 lb ft
Discharge Hose Connecting Block-to-Compressor Retaining Nut | 16 N·m | 12 lb ft
Discharge Hose Connecting Block-to-Condenser Retaining Nut | 16 N·m | 12 lb ft
ECM Bracket Mounting Nuts | 15 N·m | 11 lb ft
Evaporator Outlet Hose Clip-to-Vehicle Nut | 16 N·m | 12 lb ft
Evaporator Outlet Hose-to-Compressor Hose Nut | 16 N·m | 12 lb ft
Evaporator Outlet Hose-to-Thermal Expansion Valve Nut | 16 N·m | 12 lb ft
Front Compressor-to-Bracket Mounting Bolts | 23 N·m | 17 lb ft
HVAC Module Screws | 8 N·m | 71 lb in
HVAC Module-to-Cowl Nuts | 8 N·m | 71 lb in
Liquid Line Clip-to-Vehicle Nuts | 16 N·m | 12 lb ft
Liquid Line-to-Condenser Bolt | 14 N·m | 10 lb ft
Liquid Line-to-Thermal Expansion Valve Nut | 16 N·m | 12 lb ft
Pressure Relief Valve | 16 N·m | 12 lb ft
Pressure Transducer | 7 N·m | 62 lb in
Rear Compressor Bracket Mounting Bolts | 23 N·m | 17 lb ft
Rear Compressor-to-Bracket Mounting Bolts | 20 N·m | 15 lb ft
Thermal Expansion Valve Bolts | 10 N·m | 89 lb in
Upper Condenser Mount Bolts | 4 N·m | 35 lb in