For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim. Refer to Front Side Door Trim Panel Replacement.
2. Remove the front side door window frame rear applique. Refer to Front Door Frame Applique Replacement.
3. Remove the screws that secure the glass to the window regulator.
4. Remove the glass from the door.

### Installation Procedure

1. Install the glass in the door and position the glass within the window regulator.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the glass to the window regulator with the screws and tighten to 3 N·m (27 lb in).
3. Install the front side door window frame rear applique. Refer to Front Door Frame Applique Replacement.
4. Install the front door trim. Refer to Front Side Door Trim Panel Replacement.