For 1990-2009 cars

### Removal Procedure

1. Remove the front seat from the vehicle. Refer to Bucket Seat Replacement.
2. Remove the back panel.
3. Remove the each seat trim.
4. Disconnect the electrical connectors.
5. Remove the bolts and the seatback.

### Installation Procedure

1. Install the seatback onto the seat cushion.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the front seatback bolts.

Tighten
Tighten the front seatback bolts to 45 N·m (33 lb ft).

3. Connect the electrical connectors.
4. Install the seat trims to its original position.
5. Install the back panel onto the seat.
6. Install the front seat in the vehicle. Refer to Bucket Seat Replacement.