For 1990-2009 cars

### Circuit Description

Transmission fluid life is determined by monitoring transmission fluid temperature over a period of time. The transmission control module (TCM) calculates transmission fluid life based on a set of temperature ranges stored in TCM memory. As the vehicle is driven, a counter increments. The rate at which the counter increments depends on the temperature range in which the transmission is currently operating. The higher the temperature range, the faster the counter increments. As the counts increment, the TCM will begin to decrease the fluid life percentage from 100, high fluid life, to 0, low fluid life.

If the TCM detects a calculated transmission oil life of 10 percent or less, then DTC P0897 sets. DTC P0897 is a type C DTC.

### DTC Descriptor

This diagnostic procedure supports the following DTC:

DTC P0897 Transmission Fluid Life

### Conditions for Running the DTC

No transmission fluid temperature (TFT) DTC P0712.

### Conditions for Setting the DTC

The calculated transmission oil life remaining is 10 percent or less.

### Action Taken When the DTC Sets

• | The TCM records the operating conditions when the Conditions for Setting the DTC are met. The TCM stores this information as Failure Records.

• | The TCM stores DTC P0897 in TCM history.

### Conditions for Clearing the SVS Lamp/DTC

• | The TCM clears the DTC from TCM history if the vehicle completes 40 warm-up cycles without an emission-related diagnostic fault occurring.

• | The TCM cancels the DTC default actions when the fault no longer exists and the DTC passes.

### Diagnostic Aids

Inspect the transmission cooling system for possible blockage and restrictions.

### Test Description

The number below refers to the step number on the diagnostic table.

1. This step changes the AT fluid. It is important to reset the oil life monitor after the fluid are replaced.

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Diagnostic System Check - Vehicle? | -- | Go to Step 2 | Go to Diagnostic System Check - Vehicle
2 |

1. Install a scan tool.
2. Turn ON the ignition, with the engine OFF.

Important:

• | Before clearing the DTC, use the scan tool in order to record the PCM and the TCM Failure Records. Using the Clear Eng./Trans. DTC Info function erases the Failure Records from the powertrain control module (PCM) and the transmission control module (TCM).

• | Using the Clear Eng./Trans. DTC Info function erases stored DTCs in both the PCM and TCM.

3. Record the DTC Failure Records.
4. Clear the DTC.
5. Replace the transmission fluid. Refer to Transmission Fluid Replacement .
6. Use the scan tool in order to reset the transmission oil life.

Is the action complete?

--

Go to Step 3

--

3 | Perform the following procedure in order to verify the repair:

1. Select DTC.
2. Select Clear Info.
3. Ensure that the transmission oil life monitor displays 99 percent or greater.
4. Select Specific DTC.
5. Enter DTC P0897.

Does the DTC reset?

--

Go to Step 2

Go to Step 4

4 | With the scan tool, observe the stored information, capture info and DTC info. Does the scan tool display any DTCs that you have not diagnosed? | -- | Go to Diagnostic Trouble Code (DTC) List - Vehicle | System OK