For 1990-2009 cars

## Rear Side Door Outside Handle Replacement C100/Long Body

### Removal Procedure

1. Remove the door water deflector. Refer to Door Water Deflector Replacement .
2. Remove the outside door handle screws.
3. Remove the outside door handle screw through the door shut face.
4. Remove the outside door handle by sliding rearward and pulling away from the door.
5. Remove the gasket, if necessary.

### Installation Procedure

1. Install the gasket, if necessary.
2. Install the handle by placing into position and sliding rearward ensuring to engage the outside door handle.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the outside door handle screws.

Tighten
Tighten the outside door handle screws to 4.5 N·m (40 lb in).

4. Install the door water deflector. Refer to Door Water Deflector Replacement .

## Rear Side Door Outside Handle Replacement C105/Short Body

### Removal Procedure

1. Remove the door water deflector. Refer to Door Water Deflector Replacement .
2. Remove the rear door lock. Refer to Rear Door Lock Replacement .
3. Remove the outside door handle cover bolt.
4. Remove the outside door handle support screw .
5. Remove the outside door handle cover.
6. Slide the outside door handle knob backward and pull it outward.
7. Remove the outside door handle support.

### Installation Procedure

1. Install the outside door handle support.
2. Install the outside door handle knob.
3. Install the outside door handle cover.

Notice: Refer to Fastener Notice in the Preface section.

4. Install the outside door handle screw.

Tighten
Tighten the outside door handle screw to 4.5 N·m (40 lb in).

5. Install the outside door handle cover bolt.

Tighten
Tighten the outside door handle cover bolt to 4.5 N·m (40 lb in)

6. Install the rear door lock. Refer to Rear Door Lock Replacement .
7. Install the door water deflector. Refer to Door Water Deflector Replacement .