For 1990-2009 cars

### Removal Procedure

1. Disconnect negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the driver knee bolster. Refer to Knee Bolster Replacement .
3. Disconnect the connector of SSPS control module.
4. Remove the SSPS control module from the bracket by sliding the control module upward.
5. Remove the bracket by removing the bolts, if needed.

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the control module bracket and the bolts.

Tighten
Tighten the SSPS control module bracket bolts to 10 N·m (88.5 lb in).

2. Install the SSPS control module to the bracket.
3. Connect the connector of SSPS control module.
4. Install the driver knee bolster. Refer to Knee Bolster Replacement .
5. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .