For 1990-2009 cars

### Removal Procedure

Warning: Refer to Battery Disconnect Warning in the Preface section.

1. Disconnect the negative battery cable.
2. Remove the nut and the pedal mounting shaft.
3. Disconnect the return spring from the mount brace.
4. Remove the E-ring from the clutch pedal.
5. Remove the push rod from the clutch pedal.
6. Remove the clutch pedal.

### Installation Procedure

1. Install the clutch pedal.
2. Coat the push rod with multi-purpose grease.
3. Install the push rod to the clutch pedal.
4. Install the E-ring to the clutch pedal.
5. Coat the pedal mounting shaft with multi-purpose grease.
6. Connect the return spring to the mount brace.

Caution: Refer to Fastener Caution in the Preface section.

7. Install the nut and the pedal mounting shaft and tighten to 18 N·m (13 lb ft).
8. Connect the negative battery cable.