For 1990-2009 cars

#### Special Tools

DW-110-060 Engine Assembly Support Fixture

### Removal Procedure

Note: Only lift the engine far enough to take the weight off the transaxle front mount assembly, or damage to the mount and lifting equipment failure may occur.

1. Remove the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement
2. Remove the air cleaner assembly. Refer to Air Cleaner Assembly Replacement
3. Support the engine assembly using DW-110-060 fixture .
4. Remove the engine mount adapter retaining bolts from the engine mount support bracket.
5. Remove the engine mount frame side bracket retaining bolt and nuts.
6. Remove the engine mount assembly.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the engine mount assembly and tighten.

• | The engine mount frame side bracket retaining bolt to 100 N·m (74 lb ft).

• | The engine mount frame side bracket retaining nuts to 90 N·m (66 lb ft).

• | The engine mount adapter retaining bolts to 50 N·m (37 lb ft).

2. Remove DW-110-060 fixture .
3. Install the air cleaner assembly. Refer to Air Cleaner Assembly Replacement
4. Install the fuel injector sight shield. Refer to Fuel Injector Sight Shield Replacement