For 1990-2009 cars

### Removal Procedure

1. Remove the bolt (1) and the seat belt anchor (2) on the floor.
2. Remove the quarter window trim panel.
3. Remove the wheelhouse trim panel.
4. Remove the bolt (1) and the seat belt anchor (2).
5. Remove the bolt (1) and the seat belt retractor (2).

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the seat belt retractor (2) with the bolt (1) and tighten to 38 N·m (28 lb ft).
2. Install the seat belt anchor (2) with the bolt (1) and tighten to 38 N·m (28 lb ft).
3. Install the wheelhouse trim panel.
4. Install the quarter window trim panel.
5. Install the seat belt anchor with the bolt (1) to the floor and tighten to 38 N·m (28 lb ft).