For 1990-2009 cars

### Removal Procedure

1. Remove the engine undercover shield. Refer to Engine Shield Replacement.
2. Drain the engine oil.
3. Remove the charge air system hoses and ducts. Refer to Charge Air Cooler Inlet Pipe and Outlet Pipe Replacement.
4. Remove the oil pan flange-to-transaxle bolts.
5. Remove the A/C compressor lower bolts.
6. Remove the oil pan.

### Cleaning Procedure

1. Clean the oil pan sealing surface.
2. Clean the engine bed plate sealing surface.
3. Clean the oil pan bolts.
4. Clean the engine bed plate bolt holes.

### Installation Procedure

1. Coat the sealant (LOCTITE 5900) on the oil pan sealing surface.
2. Install the oil pan.
3. Install the A/C compressor lower bolts.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the oil pan flange-to-transaxle bolts and tighten.

• | The oil pan tightening bolts to 11 N·m (97.4 lb in).

• | The A/C compressor lower bolts to 23 N·m (17 lb ft).

• | The oil pan flange-to-transaxle bolts to 50 N·m (36.9 lb ft).

5. Install the charge air system hoses and ducts. Refer to Charge Air Cooler Inlet Pipe and Outlet Pipe Replacement.
6. Fill the engine with engine oil.
7. Install the engine undercover shield. Refer to Engine Shield Replacement.