For 1990-2009 cars

#### Vibration at Idle

Condition | Action
--- | ---
DEFINITION: Vibration at base idle.
Engine and or Transaxle mounts | Inspect the engine and or transaxle for loose, damaged or missing mounts. Repair as necessary.
Exhaust System | Inspect the complete exhaust system for proper installation and/or damage.
Drivetrain "grounded out" to or on the vehicle chassis | Inspect the compete drive-train for signs of physical contact. Correct as necessary.
Drive Axles | Inspect both drive axles for proper installation and/or damage. Repair as necessary.
Engine Flexplate | Inspect the flexplate for damage, excessive run-out. Correct as necessary.
Base Engine | Inspect the engine for any base level concerns. Repair as necessary.