For 1990-2009 cars

### Removal Procedure

Note: Left-Hand Drive Shown, Right-Hand Drive Similar.

1. Remove the hood release handle screws.
2. Remove the knee bolster and the hood release handle.
3. Remove the cable from the hood release handle.
4. Remove the hood secondary latch. Refer to Hood Primary Latch Replacement.
5. Remove the cable from the engine compartment.

### Installation Procedure

1. Install the cable through the engine compartment.
2. Install the hood secondary latch. Refer to Hood Primary Latch Replacement.
3. Install the cable to the hood release handle.

Caution: Refer to Fastener Caution in the Preface section.

4. Install the hood release handle and the knee bolster with the screw and tighten to 2 N·m (18 lb in).