For 1990-2009 cars

#### Tools Required

J 26610 (KM-J-22610) Installer

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the power steering gear assembly. Refer to Steering Gear Replacement .
3. Remove the outer tie rod. Refer to Rack and Pinion Outer Tie Rod End Replacement .
4. Remove the dust boot outer retaining clamps.
5. Cut and remove the dust boot inner retaining clamps.
6. Remove the dust boot.

### Installation procedure

1. Install the dust boot.
2. Install the dust boot outer retaining clamp.
3. Install the dust boot inner retaining clamp with the J 26610 (KM-J-22610).
4. Install the outer tie rod. Refer to Rack and Pinion Outer Tie Rod End Replacement .
5. Install the power steering gear assembly. Refer to Steering Gear Replacement .
6. Lower the vehicle.