For 1990-2009 cars

#### Tools Required

J 45201 Cooler Line Seal Remover

1. Insert the collet (2) of the J 45201 completely into the fluid cooler pipe fitting seal (87).
2. Insert the forcing screw (1) of the J 45201 into the collet (2).
3. Tighten the forcing screw (1) until snug.
4. Thread the collar (1) of the J 45201 onto the collet (3) until snug.
5. Using an adjustable wrench, turn the collar clockwise in order to remove the fluid cooler pipe fitting seal (87).
6. Discard the fluid cooler pipe fitting seal.
7. Clean the case bores for the fluid cooler pipe fitting seals as needed.