For 1990-2009 cars

#### Special Tools

DW-110-060 Engine Assembly Support Fixture

### Removal Procedure

Note: Only lift the engine far enough to take the weight off the transaxle front mount assembly.

1. Support the engine assembly using DW-110-060 fixture .
2. Remove the transaxle front mount-to-transaxle through bolt and nut.
3. Remove the transaxle front mount retaining bolts from the transaxle.
4. Remove the transaxle front mount assembly.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

Note: Before tightening the transaxle front mount through bolt and nut, swing the engine assembly backwards and forwards or from the side to side for the proper alignment.

1. Install the transaxle front mount assembly and tighten bolts to 50 N·m (37 lb ft).
2. Install the transaxle front mount through bolt and nut and tighten to 90 N·m (66 lb ft).