For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the instrument panel. Refer to Instrument Panel Assembly Replacement .
3. Remove the actuating rod by snapping the rod out of the lever with needle-nose pliers.
4. Remove the actuating lever.
5. Disconnect the electrical connector.
6. Remove the motor retaining screws.
7. Remove the motor.

### Installation Procedure

1. Install the motor.
2. Install the motor retaining bolts and tighten.
3. Install the actuating lever.
4. Install the actuating rod.
5. Connect the electrical connector.
6. Install the instrument panel. Refer to Instrument Panel Assembly Replacement .
7. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .