For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the stabilizer shaft clamp bolts.
3. Remove the insulators from the stabilizer shaft.

### Installation Procedure

1. Install the insulators the stabilizer shaft.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the stabilizer shaft clamp bolts and tighten to 70 N·m (52 lb ft).
3. Lower the vehicle.