For 1990-2009 cars

1. Install a new oil suction tube seal onto the oil suction tube.

Caution: Refer to Fastener Caution in the Preface section.

2. Install the oil suction pipe and tighten the attaching bolts.

• | Gouges or damage to the oil pan sealing surfaces,

• | Damage to the crankshaft oil deflector

• | Damage to the bolt holes

• | Damage to the oil suction tube mounting bosses

• | Damage to the crankshaft oil deflector mounting bosses

Tighten
Tighten the oil suction pipe attaching bolt to 10 N·m (89 lb in).

3. Install the crankshaft oil deflector into the oil pan assembly and tighten the attaching bolts.

Tighten
Tighten the crankshaft oil deflector into the oil pan assembly attaching bolt to 10 N·m (89 lb in).

4. Install the oil level sensor into the oil pan assembly.

Tighten
Tighten the oil level sensor to 20 N·m (15 lb ft).

5. Install the oil pan drain plug into the oil pan assembly.

Tighten
Tighten the oil pan drain plug to 25 N·m (18 lb ft).