For 1990-2009 cars

#### Tools Required

J 45404 Transmission Indicator Alignment Tool

### Removal Procedure

1. Disconnect the negative battery cable from the battery. Refer to Battery Disconnect Caution .

Important: The transaxle manual shaft must be in neutral (N) position prior to re-installing the switch.

2. Apply the parking brake and place control shift lever in neutral (N).
3. Remove the transaxle range switch lever. Refer to Transmission Range Switch Lever Replacement .
4. Disconnect the electrical connectors (3, 5) from the transaxle range switch.
5. Using a screwdriver, bend the lockwasher tabs down away from the manual shaft nut.
6. Remove the nut, lock tab washer, and flat washer.
7. Remove the transaxle range switch bolt (2), stud (1), and flat washers.
8. Remove the transaxle range switch (3).

### Installation Procedure

1. Install the transaxle range switch (3) to the manual shaft lever.
2. Install the washer stud (1) and the bolt (2). Hand tighten ONLY at this time.

Notice: Refer to Fastener Notice in the Preface section.

3. Install the flat washer, lock tab washer, and nut.

Tighten
Tighten the nut to 7 N·m (62 lb in).

4. Ensure the manual shaft is in neutral (N) position.
5. Bend the lock washer tabs up to secure the nut.
6. Install the J 45404 to the manual shaft and rotate the transaxle range switch until the neutral base line on the switch lines up with the indicator line on the J 45404 .
7. Tighten the transaxle range switch bolt and stud (76).

Tighten
Tighten the bolt and stud to 25 N·m (18 lb ft).

8. Remove the J 45404 from the manual shaft.
9. Connect the electrical connectors (3, 5) to the transaxle range switch.
10. Install the transaxle range switch lever. Refer to Transmission Range Switch Lever Replacement .
11. Connect the negative battery cable to the battery. Refer to Battery Disconnect Caution .
12. After installing and adjusting the switch, verify the engine only starts in park (P) or neutral (N). If the engine starts in any other position, readjust the switch. Refer to Transmission Range Switch Adjustment .