For 1990-2009 cars

### Removal Procedure

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the stabilizer bar clamp to cradle bolts.
3. Remove the stabilizer bar clamps and bushings from the stabilizer bar.

### Installation Procedure

1. Install the stabilizer bar clamps and bushings to the stabilizer bar.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the stabilizer bar clamp to cradle bolts.

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

3. Lower the vehicle.