For 1990-2009 cars

## Grille Replacement C100/Long Body

### Removal Procedure

1. Open the hood.
2. Remove the nuts and the radiator grille.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the radiator grille with the nuts and tighten to 4.5 N·m (40 lb in).
2. Close the hood.

## Grille Replacement C105/Short Body

### Removal Procedure

1. Open the hood.
2. Remove the nuts and the radiator grille.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the radiator grille with the nuts and tighten to 4.5 N·m (40 lb in).
2. Close the hood.