For 1990-2009 cars

### Removal Procedure

1. Remove the rear second seat assembly. Refer to Rear Number 2 Folding Seat Replacement.
2. Remove the bolt (2) and the seat belt buckle (1).

### Installation Procedure

Notice: Refer to Fastener Notice in the Preface section.

1. Install the seat belt buckle (1) and secure with bolt (2).

Tighten
Tighten the seat belt buckle bolt to 38 N·m (28 lb ft).

2. Install the rear second seat assembly. Refer to Rear Number 2 Folding Seat Replacement.