For 1990-2009 cars

### Removal Procedure

1. Remove the brake fluid reservoir-to-master cylinder pins and remove the reservoir from the master cylinder.
2. Remove the brake pipe fittings from the master cylinder.
3. Plug the brake pipe openings and the brake fluid reservoir to prevent brake fluid loss and contamination.
4. Remove the master cylinder-to-brake booster nuts.
5. Remove the master cylinder and drain the brake fluid.

### Installation Procedure

Caution: Refer to Fastener Caution in the Preface section.

1. Install the master cylinder to the brake booster and tighten to 13 N·m (115 lb in).
2. Unplug all the openings.
3. Install the brake pipe fittings to the master cylinder and tighten to 16 N·m (12 lb ft).
4. Install the brake pipe fluid reservoir-to-master cylinder pins.
5. Add the brake fluid.
6. Check for leaks.
7. Recheck the fluid level.
8. Bleed the brake system. Refer to Hydraulic Brake System Bleeding.